		
		Windows 3.1 Display Driver Support for the 
		    Compaq CL5420 Graphics Controller
			Installation Instructions

			    ** IMPORTANT **

This driver disk is designed to allow you to select or change the video 
driver for Windows 3.1 using Windows Setup. Setup can be executed from within 
Windows, or from DOS. Note that these driver files are in Microsoft compressed 
format and can only be accessed and executed by installing through Windows 
Setup.  Simply copying the files into your \Windows\System subdirectory WILL 
NOT work and may corrupt your Windows installation. Installing the drivers 
correctly is, however, a simple process.

Installing Windows 3.1 display drivers
To install the Windows 3.1 drivers from the DOS prompt, proceed as follows:
Insure that Windows 3.1 is already installed on your computer.
From your Windows directory, at the DOS prompt, type SETUP[Enter] to run 
the Windows SETUP.EXE program. Follow the instructions on the screen. 
When you come to the screen which lists the hardware and software 
components such as display adapter (e.g. VGA, CGA, etc.), keyboard type, 
mouse type, etc., go to the Display selection by using cursor keys to move 
the highlighted bar and press [Enter].
From the next menu listing of display options, scroll to the bottom of 
the list, and highlight the following text:

Other (Requires disk provided by a hardware manufacturer)
Press [Enter], and when prompted, insert the Windows Display 

Driver diskette into drive A: and type A:\[Enter].

You will see the list of drivers and their associated resolutions, such as:

Compaq/CL 5420, 1024x768x16 Large font
Compaq/CL 5420, 1024x768x16 Small font
Compaq/CL 5420, 640x480x16
Compaq/CL 5420, 640x480x256
Compaq/CL 5420, 800x600x16
Compaq/CL 5420, 800x600x256

Highlight the desired choice by moving the cursor to the correct display 
driver, and then press [Enter].
Continue with the remainder of the setup procedure.

To install the Windows 3.1 drivers from within Windows, proceed as follows:
Insure that Windows 3.1 is already installed on your computer and start 
Windows.
From the Main window of the Program Manager run the Windows 3.1 Setup program.
Select Change Systems Settings... from the Options menu of Setup.
Click on the down arrow at the right side of the Display: line. Scroll to the end of the list of 
available display drivers and select Other display (Requires disk from OEM)....
Insert the Windows display driver diskette into drive A: and type A:\[Enter] 
as the pathname, then click on OK.
You will see the list of available drivers and their associated resolutions, 
such as:

Compaq/CL 5420, 640x480x16 
Compaq/CL 5420, 800x600x16
Compaq/CL 5420, 1024x768x16 Large font
Compaq/CL 5420, 1024x768x16 Small font
Compaq/CL 5420, 640x480x256
Compaq/CL 5420, 800x600x256

Highlight by moving the cursor to the desired display driver, and then click on OK.
Continue with the remainder of the setup procedure. The changes will not take effect until Windows 
is restarted.


SetRES Utility Installation
SetRES is a utility that runs under Windows 3.x. It allows the user to change the screen resolution, 
number of screen colors, and select either large or normal fonts and system 
resources.  

After new options have been selected, the user can either 
immediately restart Windows, in which case the new resolution will take 
effect immediately, or continue working in the current resolution, in which 
case the new resolution will take effect the next time Windows is started. 

This application assumes that the Windows drivers have been correctly 
configured using Windows Setup.  For information on installing and 
configuring Windows display drivers using setup, please refer to the 
Microsoft Windows section in this manual.  
     
Installation
Start Windows.
In the Program Manager, choose File Run.
Specify the diskette drive where the Windows Drivers and Utilities Diskette 
is inserted, and run the install program. 
For instance if the floppy is 
in drive A:, type A:\INSTALL[Enter]

If you are installing from the hard drive specify the drive where the
Windows Drivers and Utilities files are located as follows:
C:\WINDOWS\SYSTEM\OPTIONS\INSTALL[Enter]

When prompted, specify the Windows directory.
Note:  This application MUST be installed in the WINDOWS directory.

SetRES may now be run by selecting the SetRES icon.
Use the SetRES utility to select supported colors and resolutions.
For help on the SetRES utility, select Help from the program menu.





